## Ocean Gate Control Centre

Ocean Gate Control Centre VTS equipment configuration includes:

VTS Processing Core

* 2 x System Server;
* 2 x Database Server;
* Recording Server;
* Video Recording Server;
* Meteo Server;
* RDF Server;
* CCTV Server;
* DSC Server;
* Time Server

Operator Workplace:

* 5x Operator Console:
  + 1 x Operator PC;
  + 3 x Traffic Display;
  + 1 x Admin Display;

**Sensors**

* Hydrologic Sensor;

**Network Equipment**

* LAN Switch;

**Auxiliary Equipment**

* Monitoring Unit.

Diagram

Description automatically generated

Figure 2‑2 Block Diagram of Server Room

Graphical user interface

Description automatically generated

Figure 2‑3 Block Diagram of Operators Room